STAY DAMPER DISPOSAL

id091100521000

  Note
  • The stay damper contains colorless, odorless, nontoxic gas.

1. Wear protective eye wear.

2. Position the stay damper horizontally.

am2zzw00000434

3. Drain gas and oil by cutting the position indicated in the figure to a 2—3 mm{0.08—0.11 in} depth using a metal saw.

  Caution
  • Be careful. The gas and oil may spray out with force.

4. Verify that the gas and oil is drained completely by pulling and pushing the piston rod several times with the cut position facing downward.

am2zzw00000435

5. Cut off the bottom of the stay damper.

ac9wzw00002491

6. Dispose of the stay damper.