HEADLIGHT LEVELING SWITCH INSPECTION

id091800803700

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Driver side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (3) Headlight leveling switch (See HEADLIGHT LEVELING SWITCH REMOVAL/INSTALLATION.)

3. Verify that the resistance and continuity between the headlight leveling switch terminals is as indicated in the table.

ac9wzw00002616

  • If not as indicated in the table, replace the headlight leveling switch.

ac9wzw00002566