STARTER REMOVAL/INSTALLATION [MZI-3.7]

id0119c2800200

  Warning
  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.
  • When the battery cables are connected, touching the vehicle body with starter terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the negative battery cable before performing the following operation.

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Position the selector cable out of the way. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

ac9wzw00001417

1 | Wiring harness bracket
2 | Terminal B cable
3 | Terminal S connector
4 | Starter