B-PILLAR UPPER TRIM REMOVAL/INSTALLATION

id091700802100

1. Remove the following parts:

  (1) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (2) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Front seat belt lower anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (4) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (5) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

2. Partially peel back the seaming welt.

ac9uuw00000331

3. Detach clips A and C, and pin B by pulling them in the direction of the arrow.

4. Remove the B pillar upper trim in the direction of the arrow.

ac9uuw00002128

5. Install in the reverse order of removal.