ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION

id040200110500

• The parameter identification (PID)/data monitor function is used for optionally selecting input/output signal monitor items preset in the dynamic stability control (DSC)/roll stability control (RSC) hydraulic unit (HU)/control module (CM) and reading them out in real-time.

PID/DATA Monitor Table

PID/data monitor item | Input/output part | Unit/Condition (Tester display)
--- | --- | ---
ACCLMTR | SAS control module | G
BOO_ABS | Brake switch | Off/On
CCNTABS | Number of continuous DTCs | —
LAT_ACCL | SAS control module (lateral-G value) | G
MCYLI P | Brake fluid pressure sensor | MPa, psi
PMP_MOTOR | Pump motor | Off/On
PWR_RLY | Valve relay | Off/On
ROLL_RATE | SAS control module | °/s
SHIFT_P | TCM | Off/On
SWA_POS | Steering angle sensor | °
TCS_OFF_SW | TCS OFF switch | Off/On
V_LF_INL | LF inlet solenoid valve | Off/On
V_LF_OTL | LF outlet solenoid valve | Off/On
V_LR_INL | LR inlet solenoid valve | Off/On
V_LR_OTL | LR outlet solenoid valve | Off/On
V_RF_INL | RF inlet solenoid valve | Off/On
V_RF_OTL | RF outlet solenoid valve | Off/On
V_RR_INL | RR inlet solenoid valve | Off/On
V_RR_OTL | RR outlet solenoid valve | Off/On
V_STB_L | LH stability control solenoid valve | Off/On
V_STB_R | RH stability control solenoid valve | Off/On
V_TRC_L | LH traction control solenoid valve | Off/On
V_TRC_R | RH traction control solenoid valve | Off/On
WSPD_LF | ABS wheel-speed sensor (LF) | KPH, MPH
WSPD_LR | ABS wheel-speed sensor (LR) | KPH, MPH
WSPD_RF | ABS wheel-speed sensor (RF) | KPH, MPH
WSPD_RR | ABS wheel-speed sensor (RR) | KPH, MPH
YAW_RATE | SAS control module (yaw rate value) | °/s