KEYLESS ANTENNA REMOVAL/INSTALLATION [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914008077z6

Exterior, LF/RF

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the screws.

ac9wzw00001183

5. Disconnect the connector, then remove the keyless antenna.

6. Install in the reverse order of removal.

Exterior, Rear

1. Disconnect the negative battery cable.

2. Remove the screws.

ac9uuw00002395

3. Disconnect the connector, then remove the keyless antenna.

4. Install in the reverse order of removal.

Interior, Front

Center

1. Disconnect the negative battery cable.

2. Remove the decoration panel. (See DECORATION PANEL REMOVAL/INSTALLATION.)

3. Remove the front console box mat. (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

4. Remove the indicator panel. (See INDICATOR PANEL REMOVAL/INSTALLATION.)

5. Remove the front console box. (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

6. Disconnect the connector, then remove the screws.

ac9uuw00001223

7. Remove the keyless antenna.

8. Install in the reverse order of removal.

Interior, Middle

1. Disconnect the negative battery cable.

2. Remove the console cover. (See CONSOLE COVER REMOVAL/INSTALLATION.)

3. Remove the clips.

ac9wzw00001184

4. Disconnect the connector, then remove the keyless antenna.

5. Install in the reverse order of removal.

Interior, Rear

1. Disconnect the negative battery cable.

2. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)

3. Remove the third-row seat. (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

4. Partially peel back the floor covering.

5. Remove the nuts.

ac9uuw00002396

6. Disconnect the connector, then remove the keyless antenna.

7. Install in the reverse order of removal.