DTC B1126 [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id09021g802600

DTC B1126 | Steering lock unit internal malfunction
--- | ---
DETECTION CONDITION | Detect the steering lock unit malfunction signal
POSSIBLE CAUSE | Steering lock unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT STEERING LOCK UNIT • Clear the DTC using the M-MDS. • Turn the ignition switch to the ON position. • Is the DTC displayed? ― M-MDS: B1126 | Yes | Replace the steering lock unit and perform the resetting procedure for the advanced keyless system when replacing the keyless control module. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.