KEYLESS RECEIVER REMOVAL/INSTALLATION

id091400807500

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Upper column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (7) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00002154

1 | Screw
2 | Keyless receiver
3 | Connector

4. Install in the reverse order of removal.