TRANSFER OIL INSPECTION

id031600800200

1. Park the vehicle on level ground.

2. Remove the filler plug.

ac9wzw00000799

3. Verify that the oil is near the brim of the filler plug hole.

  • If the oil level is low, add the specified type of oil through the filler plug hole until the level reaches the brim of the filler plug hole.

  Transfer oil

  Grade: API service GL-5
  Viscosity: SAE 75W-140

4. Apply sealant to the filler plug.

5. Tighten the filler plug before the applied sealant starts to harden.

  Tightening torque

  17—24 N·m {1.8—2.4 kgf·m, 13—17 ft·lbf}

6. Inspect for oil leakage.