AUXILIARY JACK/USB PORT INSPECTION

id092000811600

Auxiliary jack inspection

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Console cover. (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Auxiliary jack/USB port (See AUXILIARY JACK/USB PORT REMOVAL/INSTALLATION.)

3. Connect a commercially-available plug to the auxiliary jack/USB port.

ac9uuw00004607

4. Verify that the continuity between the auxiliary jack/USB port terminals is as indicated in the table.

ac5wzw00001480

  • If not as indicated in the table, replace the auxiliary jack/USB port.

USB port inspection

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Console cover. (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Auxiliary jack/USB port (See AUXILIARY JACK/USB PORT REMOVAL/INSTALLATION.)

3. Insert the pins to positions UA', UB', UC', and UD' shown in the figure from the side of the USB device insertion area for the auxiliary jack/USB port, and verify the continuity at the insertion side and terminal side of the USB device.

ac9wzw00002944

4. Verify that the continuity at the insertion side and terminal side of the USB device is as indicated in the table.

  Note
  • When inspecting the USB device insertion side, touch it with a paper clip or similar thin pin without directly inserting a tester into the terminals.

ac5wzw00005107

  • If not as indicated in the table, replace the auxiliary jack/USB port.