BRAKES TECHNICAL DATA

id045000800100

Item | Specification
--- | ---
Brake fluid type | Russian specs.: SAE J1703 or FMVSS116 DOT-3 or DOT-4 Australian, General (L.H.D.) specs.: SAE J1703 or FMVSS116 DOT-3
Brake pedal height (reference value) | L.H.D.: 206.3 mm {8.122 in} R.H.D.: 200.9 mm {7.91 in}
Brake pedal play | 2—5 mm {0.08—0.19 in}
Brake pedal-to-floor clearance (Brake pedal when depressed at 147 N {15.0 kgf, 33.0 lbf}) | 97.6 mm {3.84 in} or more
Front disc plate runout limit | 0.05 mm {0.002 in}
Minimum front disc plate thickness | 26 mm {1.03 in}
Minimum front disc plate thickness after machining using a brake lathe on-vehicle | 26.8 mm {1.06 in}
Minimum front disc pad thickness | 2.0 mm {0.08 in}
Rear disc plate runout limit | 0.05 mm {0.002 in}
Minimum rear disc plate thickness | 16 mm {0.63 in}
Minimum rear disc plate thickness after machining using a brake lathe on-vehicle | 16.8 mm {0.66 in}
Minimum rear disc pad thickness | 2.0 mm {0.08 in}
Parking brake pedal stroke when depressed at 180 N {18.4 kgf, 40.5 lbf} | 1—3 notches
Minimum parking brake shoe thickness | 1.0 mm {0.04 in}
Maximum rear disc plate inner diameter | 191.0 mm {7.52 in}

Master cylinder fluid pressure

Vacuum amount at o kPa {0 mmHg, 0 inHg}
Pedal force | Fluid pressure
--- | ---
200 N {20.4 kgf, 44.9 lbt} | 520 kPa {5.31 kgf/cm2, 75.5 psi} or more

Master cylinder fluid pressure

Vacuum amount at 66.7 kPa {500 mmHg, 19.7 inHg}
Pedal force | Fluid pressure
--- | ---
200 N {20.4 kgf, 44.9 lbt} | 9,000 kPa {91.78 kgf/cm2, 1,306 psi} or more