FRONT POWER WINDOW REGULATOR REMOVAL/INSTALLATION

id091200001100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Front door glass (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)

  (5) Power window motor (See POWER WINDOW MOTOR REMOVAL/INSTALLATION.)

3. Remove the nuts.

ac9wzw00001636

4. Insert a hand through the speaker installation hole, rotate the drum housing in the direction shown in the figure to detach the tabs from the front door module panel.

ac9wzw00001064

5. Move the front power window regulator in the direction of the arrow and remove it.

ac9uuw00002347

6. Install in the reverse order of removal.

  Caution
  • Make sure the cable does not unspool from the drum housing when installing.