DTC INSPECTION [BCM]

id0902f5345400

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. Verify the following vehicle conditions:

  • All the switches are turned off (except the ignition switch).
  • All the doors, bonnet, and liftgate are closed.
  • All the doors, and liftgate are unlocked.
  • All the seat belts are unbuckled.
  • Parking brake lever is pulled.

3. Start the engine.

4. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  (1) Select “Self Test”.

  (2) Select “Modules”.

  (3) Select “GEM”.

5. Verify the DTC according to the directions on the screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection.

6. After completion of repairs, clear all DTCs stored in the BCM. (See CLEARING DTC [BCM].)