DRIVELINE/AXLE SPECIFICATIONS

id030000100200

Item | Specification
--- | ---
Front axle
Bearing type | Angular ball bearing
Rear axle
Bearing type | Angular ball bearing
Front drive shaft
Front drive shaft joint type | Wheel side | Bell joint
Differential side | Tripod joint
Front drive shaft diameter | (mm {in}) | LH: 27.0 {1.06} RH: 30.0 {1.18}
Joint shaft diameter | (mm {in}) | 45.0 {1.77}
Rear drive shaft
Rear drive shaft joint type | Wheel side | Bell joint
Differential side | Double offset joint
Rear drive shaft diameter | (mm {in}) | 24.0 {0.94}
Rear differential
Rear and front wheel torque distribution unit | Electronic control coupling
Reduction gear | Hypoid gear
Differential gear | Straight bevel gear
Ring gear size | (Inches) | 7.35
Final gear ratio | 2.928
Gears: Number of teeth | Drive pinion | 14
Ring gear | 41
Differential oil | Type | Grade | API service GL-5
Viscosity | SAE 80W-90
Amount (Approximate quantity) | (L {US qt, lmp qt}) | 1.0 {1.1, 0.9}
Propeller shaft
Length | (mm {in}) | L1 | 658.0 {25.91}
L2 | 570.6 {22.46}
L3 | 815.9 {32.12}
Outer diameter | (mm {in}) | D1 | 75.0 {2.95}
D2 | 63.5 {2.50}
D3 | 75.0 {2.95}
Joint type | Constant velocity joint and cross-shaped joint
Constant velocity joint | Double offset joint
Transfer
Transfer oil | Type | Grade | API service GL-5
Viscosity | SAE 75W-140
Oil capacity (approx. quantity) | (L {US qt, Imp qt}) | 0.53 {0.56, 0.47}