CONDENSER REMOVAL/INSTALLATION

id092000803000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (6) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (7) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (8) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (9) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (10) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

3. Slightly bend back the headliner.

4. Remove in the order indicated in the table.

ac9uuw00001788

1 | Bolt
2 | Connector
3 | Condenser

5. Install in the reverse order of removal.