JOINT SHAFT DISASSEMBLY [4WD]

id031300801042

1. Disassemble in the order indicated in the table.

ac9uuw00001349

1 | Cover
2 | Snap ring
3 | Joint shaft (See Joint Shaft Disassembly Note.)
4 | Dust seal (axle side) (See Dust Seal (Axle Side) Disassembly Note.)
5 | Snap ring
6 | Dust seal (differential side) (See Dust Seal (Differential Side) Disassembly Note.)
7 | Bearing (See Bearing Disassembly Note.)
8 | Bearing housing

Joint Shaft Disassembly Note

1. Remove the joint shaft using a press.

ac9uuw00001342

Dust Seal (Axle Side) Disassembly Note

1. Remove the dust seal using a flathead screwdriver.

Dust Seal (Differential Side) Disassembly Note

1. Remove the dust seal using a flathead screwdriver.

Bearing Disassembly Note

1. Remove the bearing using a press and the SSTs.

ac9uuw00001343