STEERING ANGLE SENSOR INSPECTION

id091800813400

  Note
  • The steering angle sensor is integrated with the combination switch body.

1. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

2. Turn the steering wheel to the right and left, and verify that the voltage and pulses at the terminals are as shown in the figure.

  • If not as specified, replace the combination switch body.(See COMBINATION SWITCH DISASSEMBLY/ASSEMBLY )

ac9uuw00010271