REQUEST SWITCH REMOVAL/INSTALLATION [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914008079z6

Driver Side/Passenger Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Front door glass (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)

  (5) Front door module (See FRONT DOOR MODULE PANEL REMOVAL/INSTALLATION.)

3. Remove the screw A, then remove the handle seat.

ac9wzw00001926

4. Remove screw B, then remove the request switch.

Liftgate

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the liftgate side trim. (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

5. Remove the rear finisher. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

6. Press the tabs and remove the request switch.

7. Install in the reverse order of removal.

ac9uuw00000381