FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION

id091000800600

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00000865

1 | Fastener A
2 | Front energy-absorbing foam
3 | Fastener B
4 | Seal plate
5 | Bolt A
6 | Bolt B
7 | Front bumper reinforcement

4. Install in the reverse order of removal.