EXTRACTOR CHAMBER REMOVAL/INSTALLATION

id091600801500

1. Disconnect the negative battery cable.

2. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the rear bumper. (See REAR BUMPER REMOVAL/INSTALLATION.)

4. Remove the rear over fender. (See OVER FENDER REMOVAL/INSTALLATION.)

5. Remove the screws.

6. Pull the extractor chamber in the direction shown by the arrow and remove it.

ac9uuw00000490

7. Install in the reverse order of removal.