REAR BUMPER REINFORCEMENT REMOVAL/INSTALLATION

id091000800900

1. Disconnect the negative battery cable.

2. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the rear bumper. (See REAR BUMPER REMOVAL/INSTALLATION.)

4. Remove the fasteners, then remove the energy-absorbing foam.

ac9uuw00000871

5. Remove the bolts and nuts, then remove the rear bumper reinforcement.

6. Install in the reverse order of removal.