FRONT AIR MIX ACTUATOR CONSTRUCTION

id074000106100

Construction

• Installed to both the driver and passenger sides.
• Opens/closes the air mix door based on the signals from the front climate control unit to adjust the temperature.
• A potentiometer type, which allows minute and smooth changes of the door position, has been adopted.

Operation

• The front climate control unit compares the voltage detected by the potentiometer in the front air mix actuator with the target voltage.
• Operates the motor in the front air mix actuator until the detected voltage and the target voltage are equal.

ac9wzn00000322