INDIRECT ILLUMINATION REMOVAL/INSTALLATION

id091800819300

1. Disconnect the negative battery cable.

2. Remove the intruder sensor. (with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

3. Remove the front map light. (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9uuw00002104

1 | Connector
2 | Console indirect illumination

5. Install in the reverse order of removal.