DTC P060A:00, P060C:00, P061D:00 [MZI-3.7]

id0102d2900900

DTC P060A:00 DTC P060C:00 DTC P061D:00 | P060A:00: Internal control module monitoring processor performance P060C:00: Internal control module main processor performance P061D:00: Internal control module engine air mass performance
--- | ---
DETECTION CONDITION | • Indicates an error occurred in the PCM.
POSSIBLE CAUSE | • Software incompatibility issue • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT PCM FOR LATEST CALIBRATION • Program the PCM to the latest calibration. • Turn the ignition switch off. • Perform the KOEO self-test. (See KOEO/KOER SELF TEST [MZI-3.7].) • Turn the ignition switch off. • Perform the KOER self-test. (See KOEO/KOER SELF TEST [MZI-3.7].) • Use the customer information to recreate the concern. • Perform the self-test. • Are DTCs P060A:00, P060C:00 or P061D:00 present? | Yes | Go to the next step.
No | Go to Step 5.
4 | INSPECT FOR CORRECT PCM OPERATION • Disconnect all the PCM connectors. • Visually inspect for: ― Pushed out pins ― Corrosion • Connect all the PCM connectors and verify that they seat correctly. • Retrieve DTCs using the M-MDS. • Is the PENDING CODE for this DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZI-3.7].)
No | Go to the next step.
5 | VERIFY TROUBLESHOOTING OF DTC P060A:00, P060C:00 AND P061D:00 HAS BEEN COMPLETED • Verify that all disconnected connectors reconnected. • Clear the DTC from the PCM memory using the M-MDS. • Perform the KOEO or KOER self-test. (See KOEO/KOER SELF TEST [MZI-3.7].) • Retrieve DTCs using the M-MDS. • Is the PENDING CODE for this DTC present? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZI-3.7].) Go to the next step.
No | Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [MZI-3.7].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZI-3.7].)
No | Troubleshooting completed.