AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [AY6A-EL, AY6AX-EL]

id0517k3297200

  Warning
  • A hot transaxle and ATF can cause severe burns. Turn off the engine and wait until then are cool.

  Caution
  • Do not remove the blind cap because it is not a removable part.

  am6xuw00005035

  Note
  • The following procedure is for draining the ATF from the oil pan, not for complete replacement of the ATF.

1. Remove the overflow plug, and the O-ring.

am6xuw00004034

2. Remove the overflow tube, and the gasket, and drain the ATF.

am6xuw00004035

3. Install the new gasket, and overflow tube.

  Tightening torque

  24—54 N·m {2.5—5.5 kgf·m, 18—39 ft·lbf}

4. Temporarily tighten the overflow plug reusing the O-ring.

5. Adjust the ATF level. (See AUTOMATIC TRANSAXLE FLUID (ATF) LEVEL ADJUSTMENT [AY6A-EL, AY6AX-EL].)