LIGHTING SYSTEM PERSONALIZATION

id091800013300

• A personalization function has been adopted with which settings for each function can be changed.
• Refer to the workshop manual for the detailed setting procedure.

Auto Light System

Mazda Modular Diagnostic System (M-MDS) display | Function | Initial setting | Setting contents | Control module
--- | --- | --- | --- | ---
Autolamp On Setting. | Auto light sensor sensitivity can be changed. | Standard (All Other) | Standard (All Other) / Low (All Other) | Auto light/wiper control module

High Beam Control (HBC) System

Mazda Modular Diagnostic System (M-MDS) display | Function | Initial setting | Setting contents | Control module
--- | --- | --- | --- | ---
High Beam Control. | The high beam control (HBC) system can be switched between operable and inoperable. | ON | Not Adopted. / OFF / ON | Forward sensing camera (FSC)

Running Light System

Function | Initial setting | Setting contents | Control unit
--- | --- | --- | ---
The running light system function can be set. | ON (running light illumination) | OFF (running light non-illumination)/ON (running light illumination) | Auto light/wiper control module