NOISE FILTER REMOVAL/INSTALLATION

id092000806400

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the liftgate side trim. (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

ac9wzw00001232

1 | Connector
2 | Screw
3 | Bolt
4 | Noise filter

6. Install in the reverse order of removal.