ON-BOARD DIAGNOSTIC SYSTEM OUTLINE [AY6A-EL, AY6AX-EL]

id0502k1280000

Special Features

Improved serviceability | • On-board diagnostic system adopted consisting of the following functions: ― Malfunction detection function ― Fail-safe function ― Diagnostic data memory function ― Malfunction indication function ― External tester communication function ― PID/DATA monitor function ― Simulation function • Automatic transaxle warning light adopted to notify driver of transaxle malfunction • DLC-2 adopted in compliance with ISO (International Organization for Standardization) standards • CAN adopted for communication between TCM and external diagnostic tester

Block Diagram

ac9uun00000779