WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION

id091900800900

1. Disconnect the negative battery cable.

2. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

3. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9wzw00001032

1 | Windshield wiper motor Connector
2 | Bolt
3 | Windshield wiper motor

5. Install in the reverse order of removal.