REAR DOOR LATCH AND LOCK ACTUATOR REMOVAL/INSTALLATION

id091400800500

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

  (2) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Rear door glass (See REAR DOOR GLASS REMOVAL/INSTALLATION.)

  (5) Rear door module (See REAR DOOR MODULE PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00002309

1 | Connector
2 | Screw A
3 | Screw B
4 | Front door latch and lock actuator

4. Install in the reverse order of removal.