SELECTOR LEVER INSPECTION

id051800800500

1. Turn the ignition switch to the ON position. (engine OFF)

2. With the brake pedal depressed, verify that there is a “click” at each range when shifted.

L.H.D.

ac9wzw00000032

R.H.D.

ac9wzw00000027

3. Verify that the selector lever can be shifted.

4. Verify that there is a “click” at each position when shifted from P position to M range.

5. Verify that the positions of the selector lever and the indicator are aligned.

ac9wzw00002549

  • If there is any malfunction, adjust the TR switch. (See TCM REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

6. Verify that the vehicle operates in each selected range.