FRONT SASH MOLDING INSTALLATION

id091600807000

  Note
  • Double-sided adhesive tape has already been attached to the new front sash molding.

  Warning
  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

1. When installing a new front sash molding, follow the procedure below:

  (1) Remove the adhesive remaining on the body using razor.

  (2) Remove any grease or dirt from the adhesion surface of the body.

2. When reusing the front sash molding, follow the procedure below:

  (1) Remove the adhesive remaining on the front sash molding and the body using a razor.

  (2) Remove any grease or dirt from the adhesion surface of the front sash molding and the body.

  (3) Apply primer to the bonding area of the front sash molding.

  (4) Affix double-sided adhesive tape A to the front sash molding as shown in the figure.

  ac9uuw00000477

  (5) Affix double-sided adhesive tape B to the front sash molding as shown in the figure.

  ac9uuw00001141

    Note
    • As for the double-sided adhesive tape, use beta tape 5078 (1 mm {0.04 in} thickness) or equivalent.

3. Peel off the backing of the double-sided adhesive tape.

4. Hook tab A to the body in the position where tabs B align with the sash holes.

ac9uuw00000683

5. Press the front sash molding in the direction of the arrow and install tabs B to the body.

  Caution
  • Do not press the front sash molding in any place other than the rubber areas.

6. Press the front sash molding from the vehicle rear in the direction shown in the arrow and install tab C.

  Note
  • After installing the front sash molding, verify that tabs A and B are connected properly to the body.