NO.3 VEHICLE MOVES IN P POSITION, OR PARKING GEAR DOES NOT DISENGAGE WHEN P IS DISENGAGED [AY6A-EL, AY6AX-EL]

id0503k3800800

3 | Vehicle moves in P position, or parking gear does not disengage when P is disengaged
DESCRIPTION | • Vehicle rolls on a downward slope in P position. • Tires are locked when P is disengaged. Vehicle does not move in D and R position when the accelerator pedal is depressed, and the engine remains in a stalled condition.
POSSIBLE CAUSE | • Parking mechanism malfunction (May have effect on noise or shock from transaxle) • Improper adjustment of selector lever • If the vehicle moves in N position, perform No.2 “VEHICLE MOVES IN N POSITION”