FRONT BELTLINE MOLDING REMOVAL/INSTALLATION

id091600804800

Removal

1. Fully open the front door glass.

2. Disconnect the negative battery cable.

3. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

4. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

5. Remove the power outer mirror. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)

6. Remove clip A using a protective tape-wrapped flathead screwdriver.

ac9uuw00000488

7. Lift (partially peeling back) the front beltline molding in the direction of the arrow and then remove tabs B.

8. Remove the clip C.

9. Remove the front beltline molding.

Installation

1. Install the clip A.

ac9uuw00002318

2. Install the tabs B.

3. Install the clip C.

4. Install the front beltline molding.

5. Install the power outer mirror. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)

6. Install the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

7. Install the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

8. Connect the negative battery cable.