DTC INSPECTION [AUDIO AMPLIFIER]

id0902f8345400

1. Connect the M-MDS to the DLC-2.

L.H.D.

ac9uuw00000452

R.H.D.

ac9wzw00000200

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Self Test”.
  2. Select “Modules”.
  3. Select “AM”.

3. Verify the DTC according to the directions on the screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection.

4. After completion of repairs, clear all DTCs stored in the audio amplifier. (See CLEARING DTC [AUDIO AMPLIFIER].)