AUTO LIGHT/WIPER CONTROL MODULE CONFIGURATION

id091800819200

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Module Programming”.

3. Then, select items from the screen menu in the following order.

  1. Select “Programmable Module Installation”.
  2. Select “LCM”.

4. Perform the configuration according to the directions on the screen.

5. Retrieve DTCs by the M-MDS, then verify that there is no DTC present.

  • If a DTC (s) is detected, perform the applicable DTC inspection. (See DTC TABLE [AUTO LIGHT/WIPER CONTROL MODULE].)