CABIN TEMPERATURE SENSOR REMOVAL/INSTALLATION

id074000807800

L.H.D.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Driver side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (3) Console panel (LH) (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (4) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (5) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove the screw.

ac9wzw00000702

4. Remove the cabin temperature sensor cover in the direction of the arrow.

5. Remove the cabin temperature sensor.

6. Install in the reverse order of removal.

R.H.D.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Driver side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (3) Console panel (RH) (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (4) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (5) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

3. Remove the screw.

ac9wzw00000703

4. Disconnect the cabin temperature sensor connector.

5. Disconnect the hose.

6. Remove the cabin temperature sensor component.

7. Remove the cabin temperature sensor from the cabin temperature sensor cover.

8. Install in the reverse order of removal.