DTC 10

id070200802500

DTC 10 | Front evaporator temperature sensor (present)
--- | ---
POSSIBLE CAUSE | • Front evaporator temperature sensor malfunction • Open or short circuit between front evaporator temperature sensor and front climate control unit

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is resistance between terminals 2H and 2P of front climate control unit connector (16-pin) as indicated below? ― 166 ohms—32 kilohms (-30—80 °C {-22—176 °F}) ― 2.248—2.436 kilohms (15 °C {59 °F}) | Yes | Inspect the connection of the front climate control unit connector.
No | Go to the next step.
2 | • Inspect front evaporator temperature sensor. (See FRONT EVAPORATOR TEMPERATURE SENSOR INSPECTION.) • Is it okay? | Yes | Repair wiring harness.
No | Replace front evaporator temperature sensor. (See FRONT A/C UNIT DISASSEMBLY/ASSEMBLY.)