CLUSTER SWITCH REMOVAL/INSTALLATION

id091700460800

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the bonnet release lever. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

4. Pull the cluster switch in the direction of the arrow (2) shown in the figure while pressing the tab in the direction of the arrow (1) shown in the figure, detach the tab and lower panel, and then remove the cluster switch from the lower panel.

ac9wzw00002852

5. Disconnect the connector.

6. Install in the reverse order of removal.