SECOND-ROW BUCKLE REMOVAL/INSTALLATION

id081100802100

LH

1. Remove the second-row seat (LH). (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

2. Remove the bolt A.

ac9wzw00000948

3. Remove the second-row center buckle.

4. Remove the second-row seat (LH) seat cushion pad. (See SECOND-ROW SEAT DISASSEMBLY/ASSEMBLY.)

5. Remove the bolt B.

6. Remove the second-row buckle (LH).

7. Install in the reverse order of removal.

RH

1. Remove the second-row seat (RH). (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

2. Remove in bolt.

ac9wzw00000949

3. Remove the second-row buckle (RH).

4. Install in the reverse order of removal.