STEERING TECHNICAL DATA

id065000800200

Item | Specification
--- | ---
Power steering fluid type | ATF-MIII, M-V or Dexron®II
Power steering fluid capacity (approximate quantity) | 1.27 L {1.34 US qt, 1.11 lmp qt}
Oil pump fluid pressure | 11.0—11.8 MPa {113—120 kgf/cm2, 1596—1711 psi}
Gear housing fluid pressure | 11.3—11.8 MPa {116—120 kgf/cm2, 1639—1711 psi}
Steering wheel play | 0—30 mm {0—1.18 in}
Steering wheel effort | 7.8 N·m {80 kgf·cm, 58 in·lbf} max.
Steering shaft length | 211.6 mm {8.331 in}
Steering rack runout | Near point A: 0.15 mm {0.006 in} max. Near point B: 0.20 mm {0.008 in} max.
Tie-rod end rotational torque | 0.4—2.7 N·m {4.1—27.5 kgf·cm, 3.6—23.8 in·lbf} [Pull scale reading: 3.4—25.5 N {0.35—2.60 kgf, 0.8—5.7 lbf}]
Tie rod swing torque | 0.1—4.0 N·m {1.1—40 kgf·cm, 0.89—35 in·lbf} [Pull scale reading: 1.0—40.0 N {0.2—4.0 kgf, 0.23—8.99 lbf}]
Pinion shaft rotation torque | Center of rack ±90°: 1.0—1.6 N·m {1—16 kgf·cm, 8.9—14 in·lbf} [Pull scale reading: 9—13 N {1.0—1.3 kgf, 2.1—2.9 lbf}] Except center of rack ±90°: Less than 1.68 N·m {17.1kgf·cm, 14.8 in·lbf} [Pull scale reading: Less than 13.8 N {1.4 kgf, 3.1 lbf}]