REAR DOOR SPEAKER REMOVAL/INSTALLATION

id092000805000

1. Disconnect the negative battery cable.

2. Remove the inner sail garnish. (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

3. Remove the rear door trim. (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9wzw00001231

1 | Screw
2 | Rear door speaker (See Rear Door Speaker Installation Note.)
3 | Connector

5. Install in the reverse order of removal.

Rear Door Speaker Installation Note

1. Remove the speaker with the wiring harness passing through the groove of the rear door module.

ac9uuw00002223

  Caution
  • If the speaker is installed with the wiring harness out of the groove, an open circuit in the wiring harness could occur.