SUNVISOR REMOVAL/INSTALLATION

id091700801700

1. Disconnect the negative battery cable.

2. Remove the cover.

ac9uuw00002121

3. Remove the screw.

4. Rotate the sunvisor in the direction of the arrow.

5. Unhook and remove the sunvisor.

6. Disconnect the vanity mirror illumination connector.

7. Press the center adaptor tabs as shown in the figure using two tape-wrapped flathead screwdrivers, and remove the center adaptor.

ac9uuw00002122

8. Install in the reverse order of removal.