SEAT SIDE BOX REMOVAL/INSTALLATION

id091700810900

With Bose®

1. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)

2. Detach clips A and tab B by pulling them in the direction of the arrow.

ac9uuw00002118

3. Remove the seat side box.

4. Install in the reverse order of removal.

Without Bose®

1. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)

2. Detach pins by pulling them in the direction of the arrow.

3. Remove the seat side box.

ac9uuw00002119

4. Install in the reverse order of removal.