REAR FENDER PANEL REMOVAL [PANEL REPLACEMENT]

id098008744900

1. Rough cut area (A), drill the LH:103,RH:104 locations indicated by (B).

  Caution
  • Avoid cutting with a blow torch or similar tools as the insulator (shaded area) is flammable.

2. The rear fender panel and the rear pillar (inner) are joined with spot weld sealer at the tire arch line. Use a chisel or similar tool to separate the rear fender panel from the rear pillar (inner), then remove the rear fender panel.

  Note
  • Chisel is inserted because the laser welding is given as for the arrow part of the figure below and the welding is separated.

3. Remove the rear fender panel.

4. Remove the spot weld sealer using a disc grinder.

ac9uub00000064