LUMBAR SUPPORT MOTOR INSPECTION

id091300804300

1. Disconnect the lumbar support motor connector.

2. Connect battery positive voltage to lumbar support motor terminal A or B, then verify that the lumbar support motor operate as shown in the table.

ac9wzw00001246

  • If the lumbar support motor does not operate as indicated in the table, replace the Seat back frame.

Motor operation | Connection
--- | ---
B+ | GND
Forward | A | B
Backward | B | A