POWER OUTER MIRROR INSPECTION

id091200002700

Mirror Glass Adjustment

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Disconnect the power outer mirror connector.

4. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

5. Apply battery positive voltage and connect the ground to the power outer mirror terminals and inspect the power outer mirror operation.

ac9wzw00003005

  • If the power outer mirror does not operate as indicated in the table, replace the power outer mirror. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)

With Heated Mirror

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Disconnect the power outer mirror connector.

4. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

5. Verify that the continuity is as indicated in the table.

ac9wzw00003006

  • If not as indicated in the table, or if the resistance is not within the specification, replace the power outer mirror. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)

With Retractable Outer Mirror

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Disconnect the power outer mirror connector.

4. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

5. Apply battery positive voltage and connect the ground to the power outer mirror terminals and inspect the power outer mirror operation.

ac9wzw00003007

  • If the power outer mirror does not operate as indicated in the table, replace the power outer mirror. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)

With Position Memory

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Disconnect the power outer mirror connector.

4. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

5. Verify that the resistance is as indicated in the table.

ac9wzw00003008

  • If not as indicated in the table, replace the power outer mirror. (See POWER OUTER MIRROR REMOVAL/INSTALLATION.)