THEFT-DETERRENT SIREN DISASSEMBLY/ASSEMBLY

id091400004100

1. Disconnect the negative battery cable.

2. Remove the theft-deterrent siren. (See THEFT-DETERRENT SIREN REMOVAL/INSTALLATION.)

3. Remove the short wiring harness.

4. Remove the nuts.

ac9wzw00001862

5. Remove the bracket.

6. Install in the reverse order of removal. (See Theft-Deterrent Siren Assembly Note.)

Theft-Deterrent Siren Assembly Note

1. Install the theft-deterrent siren bolt ends into the bracket grooves and temporarily install the nuts with the theft-deterrent siren pressed into the bracket.

ac9wzw00001863

2. Adjust the theft-deterrent siren angle as shown in the figure.

3. Verify that the gap between A and B shown in the figure is 3 mm or more, and then tighten the nut.