GPS ANTENNA FEEDER INSPECTION

id092000802100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (2) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (3) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Car-navigation unit (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

3. Disconnect the GPS antenna connector. (See GLOBAL POSITIONING SYSTEM (GPS) ANTENNA REMOVAL/INSTALLATION.)

4. Verify that the continuity is as indicated in the table.

With car-navigation system (without display)

ac9wzw00002865

With car-navigation system (with display)

acxuuw00003354

  • If not as indicated in the table, replace the GPS antenna feeder.

acxuuw00003355