QUICK DIAGNOSTIC CHART [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]

id090361808500

ac9wzw00001861

  Caution
  • If any of the following conditions continues indefinitely, the power window motor will heat up causing the protection circuit (integrated in power window motor) to operate. If this occurs, the operation of the power window motor protection circuit temporarily disables the power windows.
    ― Continuous up and down operation of the power window.
    ― Continuously pulling up the power window switch while the window glass is fully closed.
    ― Continuously pressing the power window switch while the window glass is fully opened.
  • A malfunction in the power window system will be determined and the system will shift to malfunction mode if the power windows are operated up or down using the power window switch while the power window protection circuit is operating.
  • While the power window system is in malfunction mode, the door glass can be moved up and down normally using the manual open/close function, but they do not operate using the auto open function and exterior open/close function.
  • The power window system reverts to normal operation after performing the Power Window Initialization Procedure.

  Note
  • The exterior open/close function does not operate when the following conditions are met.
    ― Any door or liftgate is open.
    ― The ignition is switched to position other than off.
  • The auto-open/close function (the exterior open/close function) does not operate if the power window initialization procedure has been reset.
  • Depending on the temperature and battery conditions, the window may reverse on rare occasions.